# freETarget

Source Control Document: Ribbon Cable

**INTRODUCTION**

This document describes the requirements for the freeETarget flat cable used to connect the control board to the four sensors.

**DRAWING**

The ribbon cable consists of five IDC connectors and a ten-conductor ribbon as shown in Figure 1.

A diagram of a diagram of a line

Description automatically generated with medium confidence

Figure 1: Ribbon Cable Assembly

Note the orientation of the connectors. The first four connectors are on one side, and the last one is on the opposite side.