# freETarget

Resetting the Serial Number

**From the setup icon, select the Arduino or ESP32 as appropriate**

**A screenshot of a computer program

Description automatically generated**

**Connect to the target and select the ESP icon**

**A screenshot of a phone

Description automatically generated**

**You will see number scrolling.**

**A screenshot of a computer

Description automatically generated**

**In the Command box type ! then SEND**

**You will be prompted to enter the serial number.**

**In the command box type in the serial number and !. Press SEND**

**A screenshot of a computer

Description automatically generated**

**The board will reset and go into service.**